BSS ac:22:05:db:4d:5b(on wlan0)
    TSF: 212106552475 usec (2d, 10:55:06)
    freq: 2412
    beacon interval: 100 TUs
    capability: ESS Privacy ShortSlotTime RadioMeasure (0x1411)
    signal: -57.00 dBm
    last seen: 3520 ms ago
    Information elements from Probe Response frame:
    SSID: Hoeheitsgebiet
    Supported rates: 1.0* 2.0* 5.5* 11.0* 9.0 18.0 36.0 54.0 
    DS Parameter set: channel 1
    ERP: Barker_Preamble_Mode
    Extended supported rates: 6.0 12.0 24.0 48.0 
    Country: EU Environment: Indoor/Outdoor
        Channels [1 - 13] @ 20 dBm
    HT capabilities:
        Capabilities: 0x1ac
            HT20
            SM Power Save disabled
            RX HT20 SGI
            TX STBC
            RX STBC 1-stream
            Max AMSDU length: 3839 bytes
            No DSSS/CCK HT40
        Maximum RX AMPDU length 65535 bytes (exponent: 0x003)
        Minimum RX AMPDU time spacing: 4 usec (0x05)
        HT RX MCS rate indexes supported: 0-15
        HT TX MCS rate indexes are undefined
    HT operation:
         * primary channel: 1
         * secondary channel offset: no secondary
         * STA channel width: 20 MHz
         * RIFS: 0
         * HT protection: no
         * non-GF present: 1
         * OBSS non-GF present: 0
         * dual beacon: 0
         * dual CTS protection: 0
         * STBC beacon: 0
         * L-SIG TXOP Prot: 0
         * PCO active: 0
         * PCO phase: 0
    WPA:     * Version: 1
         * Group cipher: TKIP
         * Pairwise ciphers: TKIP CCMP
         * Authentication suites: PSK
    RSN:     * Version: 1
         * Group cipher: TKIP
         * Pairwise ciphers: TKIP CCMP
         * Authentication suites: PSK
         * Capabilities: 1-PTKSA-RC 1-GTKSA-RC (0x0000)
    Extended capabilities: HT Information Exchange Supported, BSS Transition
    BSS Load:
         * station count: 1
         * channel utilisation: 103/255
         * available admission capacity: 31250 [*32us]
    WMM:     * Parameter version 1
         * BE: CW 15-1023, AIFSN 3
         * BK: CW 15-1023, AIFSN 7
         * VI: CW 7-15, AIFSN 2, TXOP 3008 usec
         * VO: CW 3-7, AIFSN 2, TXOP 1504 usec
    Country: EU Environment: Indoor/Outdoor
        Channels [1 - 13] @ 16 dBm
    WPS:     * Version: 1.0
         * Wi-Fi Protected Setup State: 2 (Configured)
         * Response Type: 3 (AP)
         * UUID: 327fd200-1dd2-11b2-8601-8e4aa01a9d4a
         * Manufacturer: Ralink Technology, Corp.
         * Model: Ralink Wireless Access Point
         * Model Number: RT2860
         * Serial Number: 12345678
         * Primary Device Type: 6-0050f204-1
         * Device name: RalinkAPS
         * Config methods:
         * RF Bands: 0x1
         * Unknown TLV (0x1049, 6 bytes): 00 37 2a 00 01 20
BSS 1c:b0:44:75:42:a5(on wlan0)
    TSF: 212108020750 usec (2d, 10:55:08)
    freq: 2457
    beacon interval: 100 TUs
    capability: ESS Privacy ShortPreamble ShortSlotTime (0x0431)
    signal: -70.00 dBm
    last seen: 2050 ms ago
    Information elements from Probe Response frame:
    SSID: o2-WLAN38
    Supported rates: 9.0 18.0 36.0 54.0 1.0* 2.0 5.5 11.0 
    DS Parameter set: channel 10
    Country: DE Environment: Indoor/Outdoor
        Channels [1 - 13] @ 20 dBm
    Power constraint: 0 dB
    ERP: <no flags>
    HT capabilities:
        Capabilities: 0x2c
            HT20
            SM Power Save disabled
            RX HT20 SGI
            No RX STBC
            Max AMSDU length: 3839 bytes
            No DSSS/CCK HT40
        Maximum RX AMPDU length 32767 bytes (exponent: 0x002)
        Minimum RX AMPDU time spacing: 16 usec (0x07)
        HT RX MCS rate indexes supported: 0-15
        HT TX MCS rate indexes are undefined
    RSN:     * Version: 1
         * Group cipher: CCMP
         * Pairwise ciphers: CCMP
         * Authentication suites: PSK
         * Capabilities: 1-PTKSA-RC 1-GTKSA-RC MFP-capable (0x0080)
         * 0 PMKIDs
         * Group mgmt cipher suite: AES-128-CMAC
    Extended supported rates: 6.0 12.0 24.0 48.0 
    HT operation:
         * primary channel: 10
         * secondary channel offset: no secondary
         * STA channel width: 20 MHz
         * RIFS: 0
         * HT protection: no
         * non-GF present: 1
         * OBSS non-GF present: 0
         * dual beacon: 0
         * dual CTS protection: 0
         * STBC beacon: 0
         * L-SIG TXOP Prot: 0
         * PCO active: 0
         * PCO phase: 0
    Overlapping BSS scan params:
         * passive dwell: 20 TUs
         * active dwell: 10 TUs
         * channel width trigger scan interval: 300 s
         * scan passive total per channel: 200 TUs
         * scan active total per channel: 20 TUs
         * BSS width channel transition delay factor: 5
         * OBSS Scan Activity Threshold: 100.00 %
    Extended capabilities: HT Information Exchange Supported
    WMM:     * Parameter version 1
         * u-APSD
         * BE: CW 15-1023, AIFSN 3
         * BK: CW 15-1023, AIFSN 7
         * VI: CW 7-15, AIFSN 2, TXOP 3008 usec
         * VO: CW 3-7, AIFSN 2, TXOP 1504 usec
    WPS:     * Version: 1.0
         * Wi-Fi Protected Setup State: 2 (Configured)
         * Response Type: 3 (AP)
         * UUID: b0493afc-202d-11b2-8a5b-1cb0447542a5
         * Manufacturer: Askey
         * Model: o2 HomeBox
         * Model Number: 6741
         * Serial Number: A804016507-009096
         * Primary Device Type: 6-0050f204-1
         * Device name: o2 HomeBox 6741
         * Config methods: Keypad
         * Unknown TLV (0x1049, 6 bytes): 00 37 2a 00 01 20
BSS 34:2c:c4:34:3b:95(on wlan0)
    TSF: 212096913717 usec (2d, 10:54:56)
    freq: 2412
    beacon interval: 100 TUs
    capability: ESS Privacy ShortSlotTime RadioMeasure (0x1411)
    signal: -77.00 dBm
    last seen: 13160 ms ago
    Information elements from Probe Response frame:
    SSID: Medusa_13
    Supported rates: 1.0* 2.0* 5.5* 11.0* 9.0 18.0 36.0 54.0 
    DS Parameter set: channel 1
    ERP: Barker_Preamble_Mode
    Extended supported rates: 6.0 12.0 24.0 48.0 
    Country: EU Environment: Indoor/Outdoor
        Channels [1 - 13] @ 20 dBm
    HT capabilities:
        Capabilities: 0x1ac
            HT20
            SM Power Save disabled
            RX HT20 SGI
            TX STBC
            RX STBC 1-stream
            Max AMSDU length: 3839 bytes
            No DSSS/CCK HT40
        Maximum RX AMPDU length 65535 bytes (exponent: 0x003)
        Minimum RX AMPDU time spacing: 4 usec (0x05)
        HT RX MCS rate indexes supported: 0-15
        HT TX MCS rate indexes are undefined
    HT operation:
         * primary channel: 1
         * secondary channel offset: no secondary
         * STA channel width: 20 MHz
         * RIFS: 0
         * HT protection: no
         * non-GF present: 0
         * OBSS non-GF present: 0
         * dual beacon: 0
         * dual CTS protection: 0
         * STBC beacon: 0
         * L-SIG TXOP Prot: 0
         * PCO active: 0
         * PCO phase: 0
    WPA:     * Version: 1
         * Group cipher: TKIP
         * Pairwise ciphers: TKIP CCMP
         * Authentication suites: PSK
    RSN:     * Version: 1
         * Group cipher: TKIP
         * Pairwise ciphers: TKIP CCMP
         * Authentication suites: PSK
         * Capabilities: 1-PTKSA-RC 1-GTKSA-RC (0x0000)
    Extended capabilities: HT Information Exchange Supported, BSS Transition
    BSS Load:
         * station count: 0
         * channel utilisation: 90/255
         * available admission capacity: 31250 [*32us]
    WMM:     * Parameter version 1
         * BE: CW 15-1023, AIFSN 3
         * BK: CW 15-1023, AIFSN 7
         * VI: CW 7-15, AIFSN 2, TXOP 3008 usec
         * VO: CW 3-7, AIFSN 2, TXOP 1504 usec
    Country: EU Environment: Indoor/Outdoor
        Channels [1 - 13] @ 16 dBm
    WPS:     * Version: 1.0
         * Wi-Fi Protected Setup State: 2 (Configured)
         * Response Type: 3 (AP)
         * UUID: 314ea500-1dd2-11b2-8601-8e4aa01a9d4a
         * Manufacturer: Ralink Technology, Corp.
         * Model: Ralink Wireless Access Point
         * Model Number: RT2860
         * Serial Number: 12345678
         * Primary Device Type: 6-0050f204-1
         * Device name: RalinkAPS
         * Config methods:
         * RF Bands: 0x1
         * Unknown TLV (0x1049, 6 bytes): 00 37 2a 00 01 20
BSS ac:22:05:e6:ff:41(on wlan0)
    TSF: 212108270373 usec (2d, 10:55:08)
    freq: 2462
    beacon interval: 100 TUs
    capability: ESS Privacy RadioMeasure (0x1011)
    signal: -41.00 dBm
    last seen: 1750 ms ago
    Information elements from Probe Response frame:
    SSID: UPCCDB29F5
    Supported rates: 1.0* 2.0* 5.5* 11.0* 9.0 18.0 36.0 54.0 
    DS Parameter set: channel 11
    ERP: Barker_Preamble_Mode
    Extended supported rates: 6.0 12.0 24.0 48.0 
    Country: EU Environment: Indoor/Outdoor
        Channels [1 - 13] @ 20 dBm
    HT capabilities:
        Capabilities: 0x1ac
            HT20
            SM Power Save disabled
            RX HT20 SGI
            TX STBC
            RX STBC 1-stream
            Max AMSDU length: 3839 bytes
            No DSSS/CCK HT40
        Maximum RX AMPDU length 65535 bytes (exponent: 0x003)
        Minimum RX AMPDU time spacing: 4 usec (0x05)
        HT RX MCS rate indexes supported: 0-15
        HT TX MCS rate indexes are undefined
    HT operation:
         * primary channel: 11
         * secondary channel offset: no secondary
         * STA channel width: 20 MHz
         * RIFS: 0
         * HT protection: no
         * non-GF present: 1
         * OBSS non-GF present: 0
         * dual beacon: 0
         * dual CTS protection: 0
         * STBC beacon: 0
         * L-SIG TXOP Prot: 0
         * PCO active: 0
         * PCO phase: 0
    WPA:     * Version: 1
         * Group cipher: TKIP
         * Pairwise ciphers: TKIP CCMP
         * Authentication suites: PSK
    RSN:     * Version: 1
         * Group cipher: TKIP
         * Pairwise ciphers: TKIP CCMP
         * Authentication suites: PSK
         * Capabilities: 1-PTKSA-RC 1-GTKSA-RC (0x0000)
    Extended capabilities: HT Information Exchange Supported, BSS Transition
    BSS Load:
         * station count: 3
         * channel utilisation: 87/255
         * available admission capacity: 31250 [*32us]
    WMM:     * Parameter version 1
         * BE: CW 15-1023, AIFSN 3
         * BK: CW 15-1023, AIFSN 7
         * VI: CW 7-15, AIFSN 2, TXOP 3008 usec
         * VO: CW 3-7, AIFSN 2, TXOP 1504 usec
    Country: EU Environment: Indoor/Outdoor
        Channels [1 - 13] @ 16 dBm
    WPS:     * Version: 1.0
         * Wi-Fi Protected Setup State: 2 (Configured)
         * Response Type: 3 (AP)
         * UUID: 314ea500-1dd2-11b2-8601-8e4aa01a9d4a
         * Manufacturer: Ralink Technology, Corp.
         * Model: Ralink Wireless Access Point
         * Model Number: RT2860
         * Serial Number: 12345678
         * Primary Device Type: 6-0050f204-1
         * Device name: RalinkAPS
         * Config methods:
         * RF Bands: 0x1
         * Unknown TLV (0x1049, 6 bytes): 00 37 2a 00 01 20
BSS ac:22:05:e6:ff:24(on wlan0) -- associated
    TSF: 212107576616 usec (2d, 10:55:07)
    freq: 5180
    beacon interval: 100 TUs
    capability: ESS Privacy ShortPreamble SpectrumMgmt ShortSlotTime RadioMeasure (0x1531)
    signal: -30.00 dBm
    last seen: 130 ms ago
    Information elements from Probe Response frame:
    SSID: UPCCDB29F5
    Supported rates: 6.0* 9.0 12.0* 18.0 24.0* 36.0 48.0 54.0 
    DS Parameter set: channel 36
    Power constraint: 3 dB
    RSN:     * Version: 1
         * Group cipher: TKIP
         * Pairwise ciphers: CCMP
         * Authentication suites: PSK
         * Capabilities: 1-PTKSA-RC 1-GTKSA-RC (0x0000)
    HT capabilities:
        Capabilities: 0x6f
            RX LDPC
            HT20/HT40
            SM Power Save disabled
            RX HT20 SGI
            RX HT40 SGI
            No RX STBC
            Max AMSDU length: 3839 bytes
            No DSSS/CCK HT40
        Maximum RX AMPDU length 65535 bytes (exponent: 0x003)
        Minimum RX AMPDU time spacing: 4 usec (0x05)
        HT RX MCS rate indexes supported: 0-23, 32
        HT TX MCS rate indexes are undefined
    HT operation:
         * primary channel: 36
         * secondary channel offset: above
         * STA channel width: any
         * RIFS: 0
         * HT protection: no
         * non-GF present: 1
         * OBSS non-GF present: 0
         * dual beacon: 0
         * dual CTS protection: 0
         * STBC beacon: 0
         * L-SIG TXOP Prot: 0
         * PCO active: 0
         * PCO phase: 0
    Extended capabilities: 6
    VHT capabilities:
        VHT Capabilities (0x33827930):
            Max MPDU length: 3895
            Supported Channel Width: neither 160 nor 80+80
            RX LDPC
            short GI (80 MHz)
            SU Beamformer
            SU Beamformee
            RX antenna pattern consistency
            TX antenna pattern consistency
        VHT RX MCS set:
            1 streams: MCS 0-9
            2 streams: MCS 0-9
            3 streams: MCS 0-9
            4 streams: not supported
            5 streams: not supported
            6 streams: not supported
            7 streams: not supported
            8 streams: not supported
        VHT RX highest supported: 0 Mbps
        VHT TX MCS set:
            1 streams: MCS 0-9
            2 streams: MCS 0-9
            3 streams: MCS 0-9
            4 streams: not supported
            5 streams: not supported
            6 streams: not supported
            7 streams: not supported
            8 streams: not supported
        VHT TX highest supported: 0 Mbps
    VHT operation:
         * channel width: 1 (80 MHz)
         * center freq segment 1: 42
         * center freq segment 2: 0
         * VHT basic MCS set: 0xffc0
    BSS Load:
         * station count: 3
         * channel utilisation: 35/255
         * available admission capacity: 30000 [*32us]
    WPA:     * Version: 1
         * Group cipher: TKIP
         * Pairwise ciphers: TKIP
         * Authentication suites: PSK
    WMM:     * Parameter version 1
         * u-APSD
         * BE: CW 15-1023, AIFSN 3
         * BK: CW 15-1023, AIFSN 7
         * VI: CW 7-15, AIFSN 2, TXOP 3008 usec
         * VO: CW 3-7, AIFSN 2, TXOP 1504 usec
    WPS:     * Version: 1.0
         * Wi-Fi Protected Setup State: 2 (Configured)
         * Response Type: 3 (AP)
         * UUID: 314ea500-1dd2-11b2-8601-8e4aa01a9d4a
         * Manufacturer: Marvell
         * Model: WAP
         * Model Number: 123
         * Serial Number: 12345
         * Primary Device Type: 6-0050f204-1
         * Device name: 5G wireless AP
         * Config methods:
         * RF Bands: 0x2
         * Unknown TLV (0x1049, 6 bytes): 00 37 2a 00 01 20
BSS a8:d3:f7:96:10:69(on wlan0)
    TSF: 212107440363 usec (2d, 10:55:07)
    freq: 2442
    beacon interval: 100 TUs
    capability: ESS Privacy ShortPreamble ShortSlotTime (0x0431)
    signal: -81.00 dBm
    last seen: 2630 ms ago
    Information elements from Probe Response frame:
    SSID: o2-WLAN34
    Supported rates: 9.0 18.0 36.0 54.0 1.0* 2.0 5.5 11.0 
    DS Parameter set: channel 7
    Country: DE Environment: Indoor/Outdoor
        Channels [1 - 13] @ 20 dBm
    Power constraint: 0 dB
    ERP: <no flags>
    HT capabilities:
        Capabilities: 0x2c
            HT20
            SM Power Save disabled
            RX HT20 SGI
            No RX STBC
            Max AMSDU length: 3839 bytes
            No DSSS/CCK HT40
        Maximum RX AMPDU length 32767 bytes (exponent: 0x002)
        Minimum RX AMPDU time spacing: 16 usec (0x07)
        HT RX MCS rate indexes supported: 0-15
        HT TX MCS rate indexes are undefined
    RSN:     * Version: 1
         * Group cipher: CCMP
         * Pairwise ciphers: CCMP
         * Authentication suites: PSK
         * Capabilities: 1-PTKSA-RC 1-GTKSA-RC (0x0000)
    Extended supported rates: 6.0 12.0 24.0 48.0 
    HT operation:
         * primary channel: 7
         * secondary channel offset: no secondary
         * STA channel width: 20 MHz
         * RIFS: 0
         * HT protection: nonmember
         * non-GF present: 1
         * OBSS non-GF present: 0
         * dual beacon: 0
         * dual CTS protection: 0
         * STBC beacon: 0
         * L-SIG TXOP Prot: 0
         * PCO active: 0
         * PCO phase: 0
    Overlapping BSS scan params:
         * passive dwell: 20 TUs
         * active dwell: 10 TUs
         * channel width trigger scan interval: 300 s
         * scan passive total per channel: 200 TUs
         * scan active total per channel: 20 TUs
         * BSS width channel transition delay factor: 5
         * OBSS Scan Activity Threshold: 100.00 %
    Extended capabilities: HT Information Exchange Supported
    WMM:     * Parameter version 1
         * u-APSD
         * BE: CW 15-1023, AIFSN 3
         * BK: CW 15-1023, AIFSN 7
         * VI: CW 7-15, AIFSN 2, TXOP 3008 usec
         * VO: CW 3-7, AIFSN 2, TXOP 1504 usec
    WPS:     * Version: 1.0
         * Wi-Fi Protected Setup State: 2 (Configured)
         * Response Type: 3 (AP)
         * UUID: 4e9bd57c-8ebe-46d8-aa04-cdd3994f7288
         * Manufacturer: Arcadyan
         * Model: o2 HomeBox 6441
         * Model Number: IAD 6441
         * Serial Number: D512146595
         * Primary Device Type: 6-0050f204-1
         * Device name: D512146595-A8D3F7
         * Config methods:
         * RF Bands: 0x3
         * Unknown TLV (0x1049, 6 bytes): 00 37 2a 00 01 20
BSS 54:fa:3e:87:1f:93(on wlan0)
    TSF: 212108698335 usec (2d, 10:55:08)
    freq: 2472
    beacon interval: 100 TUs
    capability: ESS Privacy ShortSlotTime APSD (0x0c11)
    signal: -72.00 dBm
    last seen: 1310 ms ago
    Information elements from Probe Response frame:
    SSID: moin moin
    Supported rates: 1.0* 2.0* 5.5* 11.0* 9.0 18.0 36.0 54.0 
    DS Parameter set: channel 13
    ERP: Barker_Preamble_Mode
    Extended supported rates: 6.0 12.0 24.0 48.0 
    HT capabilities:
        Capabilities: 0x1ec
            HT20
            SM Power Save disabled
            RX HT20 SGI
            RX HT40 SGI
            TX STBC
            RX STBC 1-stream
            Max AMSDU length: 3839 bytes
            No DSSS/CCK HT40
        Maximum RX AMPDU length 65535 bytes (exponent: 0x003)
        Minimum RX AMPDU time spacing: No restriction (0x00)
        HT RX MCS rate indexes supported: 0-15
        HT TX MCS rate indexes are undefined
    HT operation:
         * primary channel: 13
         * secondary channel offset: no secondary
         * STA channel width: 20 MHz
         * RIFS: 0
         * HT protection: no
         * non-GF present: 1
         * OBSS non-GF present: 0
         * dual beacon: 0
         * dual CTS protection: 0
         * STBC beacon: 0
         * L-SIG TXOP Prot: 0
         * PCO active: 0
         * PCO phase: 0
    WPA:     * Version: 1
         * Group cipher: TKIP
         * Pairwise ciphers: TKIP CCMP
         * Authentication suites: PSK
    RSN:     * Version: 1
         * Group cipher: TKIP
         * Pairwise ciphers: TKIP CCMP
         * Authentication suites: PSK
         * Capabilities: 1-PTKSA-RC 1-GTKSA-RC (0x0000)
    WMM:     * Parameter version 1
         * u-APSD
         * BE: CW 15-1023, AIFSN 3
         * BK: CW 15-1023, AIFSN 7
         * VI: CW 7-15, AIFSN 2, TXOP 3008 usec
         * VO: CW 3-7, AIFSN 2, TXOP 1504 usec
    BSS Load:
         * station count: 1
         * channel utilisation: 26/255
         * available admission capacity: 31250 [*32us]
    Extended capabilities: HT Information Exchange Supported
    Country: DE Environment: Indoor/Outdoor
        Channels [1 - 13] @ 16 dBm
    WPS:     * Version: 1.0
         * Wi-Fi Protected Setup State: 2 (Configured)
         * Response Type: 3 (AP)
         * UUID: bc329e00-1dd8-11b2-8601-54fa3e871f93
         * Manufacturer: Celeno Communication, Inc.
         * Model: Celeno Wireless AP 2.4G
         * Model Number: CL1800
         * Serial Number: 12345678
         * Primary Device Type: 6-0050f204-1
         * Device name: CelenoAP2.4G
         * Config methods: Display, PBC, Keypad
         * RF Bands: 0x1
         * Unknown TLV (0x1049, 6 bytes): 00 37 2a 00 01 20
BSS ae:22:15:db:4d:5b(on wlan0)
    TSF: 212106562854 usec (2d, 10:55:06)
    freq: 2412
    beacon interval: 100 TUs
    capability: ESS ShortSlotTime RadioMeasure (0x1401)
    signal: -57.00 dBm
    last seen: 3510 ms ago
    Information elements from Probe Response frame:
    SSID: Vodafone Hotspot
    Supported rates: 1.0* 2.0* 5.5* 11.0* 9.0 18.0 36.0 54.0 
    DS Parameter set: channel 1
    ERP: Barker_Preamble_Mode
    Extended supported rates: 6.0 12.0 24.0 48.0 
    Country: EU Environment: Indoor/Outdoor
        Channels [1 - 13] @ 20 dBm
    HT capabilities:
        Capabilities: 0x1ac
            HT20
            SM Power Save disabled
            RX HT20 SGI
            TX STBC
            RX STBC 1-stream
            Max AMSDU length: 3839 bytes
            No DSSS/CCK HT40
        Maximum RX AMPDU length 65535 bytes (exponent: 0x003)
        Minimum RX AMPDU time spacing: 4 usec (0x05)
        HT RX MCS rate indexes supported: 0-15
        HT TX MCS rate indexes are undefined
    HT operation:
         * primary channel: 1
         * secondary channel offset: no secondary
         * STA channel width: 20 MHz
         * RIFS: 0
         * HT protection: no
         * non-GF present: 1
         * OBSS non-GF present: 0
         * dual beacon: 0
         * dual CTS protection: 0
         * STBC beacon: 0
         * L-SIG TXOP Prot: 0
         * PCO active: 0
         * PCO phase: 0
    Extended capabilities: HT Information Exchange Supported, BSS Transition
    BSS Load:
         * station count: 1
         * channel utilisation: 103/255
         * available admission capacity: 31250 [*32us]
    WMM:     * Parameter version 1
         * BE: CW 15-1023, AIFSN 3
         * BK: CW 15-1023, AIFSN 7
         * VI: CW 7-15, AIFSN 2, TXOP 3008 usec
         * VO: CW 3-7, AIFSN 2, TXOP 1504 usec
    Country: EU Environment: Indoor/Outdoor
        Channels [1 - 13] @ 16 dBm
BSS 90:5c:44:d1:34:2f(on wlan0)
    TSF: 212107263738 usec (2d, 10:55:07)
    freq: 2437
    beacon interval: 100 TUs
    capability: ESS Privacy ShortSlotTime RadioMeasure (0x1411)
    signal: -53.00 dBm
    last seen: 2810 ms ago
    SSID: UPC5144FAF
    Supported rates: 1.0* 2.0* 5.5* 11.0* 9.0 18.0 36.0 54.0 
    DS Parameter set: channel 6
    ERP: Barker_Preamble_Mode
    Extended supported rates: 6.0 12.0 24.0 48.0 
    Country: EU Environment: Indoor/Outdoor
        Channels [1 - 13] @ 20 dBm
    HT capabilities:
        Capabilities: 0x1ac
            HT20
            SM Power Save disabled
            RX HT20 SGI
            TX STBC
            RX STBC 1-stream
            Max AMSDU length: 3839 bytes
            No DSSS/CCK HT40
        Maximum RX AMPDU length 65535 bytes (exponent: 0x003)
        Minimum RX AMPDU time spacing: 4 usec (0x05)
        HT RX MCS rate indexes supported: 0-15
        HT TX MCS rate indexes are undefined
    HT operation:
         * primary channel: 6
         * secondary channel offset: no secondary
         * STA channel width: 20 MHz
         * RIFS: 0
         * HT protection: non-HT mixed
         * non-GF present: 1
         * OBSS non-GF present: 0
         * dual beacon: 0
         * dual CTS protection: 0
         * STBC beacon: 0
         * L-SIG TXOP Prot: 0
         * PCO active: 0
         * PCO phase: 0
    WPA:     * Version: 1
         * Group cipher: TKIP
         * Pairwise ciphers: TKIP CCMP
         * Authentication suites: PSK
    RSN:     * Version: 1
         * Group cipher: TKIP
         * Pairwise ciphers: TKIP CCMP
         * Authentication suites: PSK
         * Capabilities: 1-PTKSA-RC 1-GTKSA-RC (0x0000)
    Extended capabilities: HT Information Exchange Supported, BSS Transition
    BSS Load:
         * station count: 1
         * channel utilisation: 109/255
         * available admission capacity: 31250 [*32us]
    WMM:     * Parameter version 1
         * BE: CW 15-1023, AIFSN 3
         * BK: CW 15-1023, AIFSN 7
         * VI: CW 7-15, AIFSN 2, TXOP 3008 usec
         * VO: CW 3-7, AIFSN 2, TXOP 1504 usec
    Country: EU Environment: Indoor/Outdoor
        Channels [1 - 13] @ 16 dBm
    WPS:     * Version: 1.0
         * Wi-Fi Protected Setup State: 2 (Configured)
         * Response Type: 3 (AP)
         * UUID: 30b60e80-1dd2-11b2-8601-8e4aa01a9d4a
         * Manufacturer: Ralink Technology, Corp.
         * Model: Ralink Wireless Access Point
         * Model Number: RT2860
         * Serial Number: 12345678
         * Primary Device Type: 6-0050f204-1
         * Device name: RalinkAPS
         * Config methods:
         * RF Bands: 0x1
         * Unknown TLV (0x1049, 6 bytes): 00 37 2a 00 01 20
BSS 92:5c:14:d1:34:2f(on wlan0)
    TSF: 212107270871 usec (2d, 10:55:07)
    freq: 2437
    beacon interval: 100 TUs
    capability: ESS ShortSlotTime RadioMeasure (0x1401)
    signal: -53.00 dBm
    last seen: 2800 ms ago
    Information elements from Probe Response frame:
    SSID: Vodafone Hotspot
    Supported rates: 1.0* 2.0* 5.5* 11.0* 9.0 18.0 36.0 54.0 
    DS Parameter set: channel 6
    ERP: Barker_Preamble_Mode
    Extended supported rates: 6.0 12.0 24.0 48.0 
    Country: EU Environment: Indoor/Outdoor
        Channels [1 - 13] @ 20 dBm
    HT capabilities:
        Capabilities: 0x1ac
            HT20
            SM Power Save disabled
            RX HT20 SGI
            TX STBC
            RX STBC 1-stream
            Max AMSDU length: 3839 bytes
            No DSSS/CCK HT40
        Maximum RX AMPDU length 65535 bytes (exponent: 0x003)
        Minimum RX AMPDU time spacing: 4 usec (0x05)
        HT RX MCS rate indexes supported: 0-15
        HT TX MCS rate indexes are undefined
    HT operation:
         * primary channel: 6
         * secondary channel offset: no secondary
         * STA channel width: 20 MHz
         * RIFS: 0
         * HT protection: non-HT mixed
         * non-GF present: 1
         * OBSS non-GF present: 0
         * dual beacon: 0
         * dual CTS protection: 0
         * STBC beacon: 0
         * L-SIG TXOP Prot: 0
         * PCO active: 0
         * PCO phase: 0
    Extended capabilities: HT Information Exchange Supported, BSS Transition
    BSS Load:
         * station count: 1
         * channel utilisation: 109/255
         * available admission capacity: 31250 [*32us]
    WMM:     * Parameter version 1
         * BE: CW 15-1023, AIFSN 3
         * BK: CW 15-1023, AIFSN 7
         * VI: CW 7-15, AIFSN 2, TXOP 3008 usec
         * VO: CW 3-7, AIFSN 2, TXOP 1504 usec
    Country: EU Environment: Indoor/Outdoor
        Channels [1 - 13] @ 16 dBm
BSS 36:2c:b4:34:3b:95(on wlan0)
    TSF: 212075883822 usec (2d, 10:54:35)
    freq: 2412
    beacon interval: 100 TUs
    capability: ESS Privacy ShortSlotTime RadioMeasure (0x1411)
    signal: -77.00 dBm
    last seen: 13150 ms ago
    Information elements from Probe Response frame:
    SSID: Gast_Medusa_13
    Supported rates: 1.0* 2.0* 5.5* 11.0* 9.0 18.0 36.0 54.0 
    DS Parameter set: channel 1
    ERP: Barker_Preamble_Mode
    Extended supported rates: 6.0 12.0 24.0 48.0 
    Country: EU Environment: Indoor/Outdoor
        Channels [1 - 13] @ 20 dBm
    HT capabilities:
        Capabilities: 0x1ac
            HT20
            SM Power Save disabled
            RX HT20 SGI
            TX STBC
            RX STBC 1-stream
            Max AMSDU length: 3839 bytes
            No DSSS/CCK HT40
        Maximum RX AMPDU length 65535 bytes (exponent: 0x003)
        Minimum RX AMPDU time spacing: 4 usec (0x05)
        HT RX MCS rate indexes supported: 0-15
        HT TX MCS rate indexes are undefined
    HT operation:
         * primary channel: 1
         * secondary channel offset: no secondary
         * STA channel width: 20 MHz
         * RIFS: 0
         * HT protection: no
         * non-GF present: 0
         * OBSS non-GF present: 0
         * dual beacon: 0
         * dual CTS protection: 0
         * STBC beacon: 0
         * L-SIG TXOP Prot: 0
         * PCO active: 0
         * PCO phase: 0
    WPA:     * Version: 1
         * Group cipher: TKIP
         * Pairwise ciphers: TKIP CCMP
         * Authentication suites: PSK
    RSN:     * Version: 1
         * Group cipher: TKIP
         * Pairwise ciphers: TKIP CCMP
         * Authentication suites: PSK
         * Capabilities: 1-PTKSA-RC 1-GTKSA-RC (0x0000)
    Extended capabilities: HT Information Exchange Supported, BSS Transition
    BSS Load:
         * station count: 0
         * channel utilisation: 94/255
         * available admission capacity: 31250 [*32us]
    WMM:     * Parameter version 1
         * BE: CW 15-1023, AIFSN 3
         * BK: CW 15-1023, AIFSN 7
         * VI: CW 7-15, AIFSN 2, TXOP 3008 usec
         * VO: CW 3-7, AIFSN 2, TXOP 1504 usec
    Country: EU Environment: Indoor/Outdoor
        Channels [1 - 13] @ 16 dBm
BSS fe:49:2d:20:d8:21(on wlan0)
    TSF: 212080903764 usec (2d, 10:54:40)
    freq: 2412
    beacon interval: 100 TUs
    capability: ESS Privacy ShortSlotTime (0x0411)
    signal: -67.00 dBm
    last seen: 29170 ms ago
    Information elements from Probe Response frame:
    SSID: \x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00\x00
    Supported rates: 6.0* 9.0 12.0* 18.0 24.0* 36.0 48.0 54.0 
    DS Parameter set: channel 1
    TIM: DTIM Count 1 DTIM Period 2 Bitmap Control 0x0 Bitmap[0] 0x0
    ERP: <no flags>
    RSN:     * Version: 1
         * Group cipher: CCMP
         * Pairwise ciphers: CCMP
         * Authentication suites: PSK
         * Capabilities: 16-PTKSA-RC 1-GTKSA-RC (0x000c)
    HT capabilities:
        Capabilities: 0x1ad
            RX LDPC
            HT20
            SM Power Save disabled
            RX HT20 SGI
            TX STBC
            RX STBC 1-stream
            Max AMSDU length: 3839 bytes
            No DSSS/CCK HT40
        Maximum RX AMPDU length 65535 bytes (exponent: 0x003)
        Minimum RX AMPDU time spacing: 4 usec (0x05)
        HT RX MCS rate indexes supported: 0-15
        HT TX MCS rate indexes are undefined
    HT operation:
         * primary channel: 1
         * secondary channel offset: no secondary
         * STA channel width: 20 MHz
         * RIFS: 1
         * HT protection: no
         * non-GF present: 0
         * OBSS non-GF present: 0
         * dual beacon: 0
         * dual CTS protection: 0
         * STBC beacon: 0
         * L-SIG TXOP Prot: 0
         * PCO active: 0
         * PCO phase: 0
    Extended capabilities: Extended Channel Switching
    WPS:     * Version: 1.0
         * Wi-Fi Protected Setup State: 2 (Configured)
         * Unknown TLV (0x1049, 6 bytes): 00 37 2a 00 01 20
         * Device name: Marion,Laura,Larissas Fire TV...
         * Primary Device Type: 1-0050f204-9
    WMM:     * Parameter version 1
         * u-APSD
         * BE: CW 15-1023, AIFSN 3
         * BK: CW 15-1023, AIFSN 7
         * VI: CW 7-15, AIFSN 2, TXOP 3008 usec
         * VO: CW 3-7, AIFSN 2, TXOP 1504 usec
    P2P:     * Group capa: 0x25, Device capa: 0xab
         * Unknown TLV (0x03, 6 bytes): 49 2d 20 58 21 dd
BSS 90:5c:44:db:21:48(on wlan0)
    TSF: 212077364612 usec (2d, 10:54:37)
    freq: 2462
    beacon interval: 100 TUs
    capability: ESS Privacy ShortSlotTime RadioMeasure (0x1411)
    signal: -76.00 dBm
    last seen: 27640 ms ago
    Information elements from Probe Response frame:
    SSID: UPC614F5E5
    Supported rates: 1.0* 2.0* 5.5* 11.0* 9.0 18.0 36.0 54.0 
    DS Parameter set: channel 11
    ERP: Barker_Preamble_Mode
    Extended supported rates: 6.0 12.0 24.0 48.0 
    Country: EU Environment: Indoor/Outdoor
        Channels [1 - 13] @ 20 dBm
    HT capabilities:
        Capabilities: 0x1ac
            HT20
            SM Power Save disabled
            RX HT20 SGI
            TX STBC
            RX STBC 1-stream
            Max AMSDU length: 3839 bytes
            No DSSS/CCK HT40
        Maximum RX AMPDU length 65535 bytes (exponent: 0x003)
        Minimum RX AMPDU time spacing: 4 usec (0x05)
        HT RX MCS rate indexes supported: 0-15
        HT TX MCS rate indexes are undefined
    HT operation:
         * primary channel: 11
         * secondary channel offset: no secondary
         * STA channel width: 20 MHz
         * RIFS: 0
         * HT protection: no
         * non-GF present: 1
         * OBSS non-GF present: 0
         * dual beacon: 0
         * dual CTS protection: 0
         * STBC beacon: 0
         * L-SIG TXOP Prot: 0
         * PCO active: 0
         * PCO phase: 0
    WPA:     * Version: 1
         * Group cipher: TKIP
         * Pairwise ciphers: TKIP CCMP
         * Authentication suites: PSK
    RSN:     * Version: 1
         * Group cipher: TKIP
         * Pairwise ciphers: TKIP CCMP
         * Authentication suites: PSK
         * Capabilities: 1-PTKSA-RC 1-GTKSA-RC (0x0000)
    Extended capabilities: HT Information Exchange Supported, BSS Transition
    BSS Load:
         * station count: 1
         * channel utilisation: 100/255
         * available admission capacity: 31250 [*32us]
    WMM:     * Parameter version 1
         * BE: CW 15-1023, AIFSN 3
         * BK: CW 15-1023, AIFSN 7
         * VI: CW 7-15, AIFSN 2, TXOP 3008 usec
         * VO: CW 3-7, AIFSN 2, TXOP 1504 usec
    Country: EU Environment: Indoor/Outdoor
        Channels [1 - 13] @ 16 dBm
    WPS:     * Version: 1.0
         * Wi-Fi Protected Setup State: 2 (Configured)
         * Response Type: 3 (AP)
         * UUID: 314ea500-1dd2-11b2-8601-8e4aa01a9d4a
         * Manufacturer: Ralink Technology, Corp.
         * Model: Ralink Wireless Access Point
         * Model Number: RT2860
         * Serial Number: 12345678
         * Primary Device Type: 6-0050f204-1
         * Device name: RalinkAPS
         * Config methods:
         * RF Bands: 0x1
         * Unknown TLV (0x1049, 6 bytes): 00 37 2a 00 01 20
BSS ae:22:15:e6:ff:41(on wlan0)
    TSF: 212108278788 usec (2d, 10:55:08)
    freq: 2462
    beacon interval: 100 TUs
    capability: ESS RadioMeasure (0x1001)
    signal: -40.00 dBm
    last seen: 1740 ms ago
    Information elements from Probe Response frame:
    SSID: Vodafone Hotspot
    Supported rates: 1.0* 2.0* 5.5* 11.0* 9.0 18.0 36.0 54.0 
    DS Parameter set: channel 11
    ERP: Barker_Preamble_Mode
    Extended supported rates: 6.0 12.0 24.0 48.0 
    Country: EU Environment: Indoor/Outdoor
        Channels [1 - 13] @ 20 dBm
    HT capabilities:
        Capabilities: 0x1ac
            HT20
            SM Power Save disabled
            RX HT20 SGI
            TX STBC
            RX STBC 1-stream
            Max AMSDU length: 3839 bytes
            No DSSS/CCK HT40
        Maximum RX AMPDU length 65535 bytes (exponent: 0x003)
        Minimum RX AMPDU time spacing: 4 usec (0x05)
        HT RX MCS rate indexes supported: 0-15
        HT TX MCS rate indexes are undefined
    HT operation:
         * primary channel: 11
         * secondary channel offset: no secondary
         * STA channel width: 20 MHz
         * RIFS: 0
         * HT protection: no
         * non-GF present: 1
         * OBSS non-GF present: 0
         * dual beacon: 0
         * dual CTS protection: 0
         * STBC beacon: 0
         * L-SIG TXOP Prot: 0
         * PCO active: 0
         * PCO phase: 0
    Extended capabilities: HT Information Exchange Supported, BSS Transition
    BSS Load:
         * station count: 3
         * channel utilisation: 87/255
         * available admission capacity: 31250 [*32us]
    WMM:     * Parameter version 1
         * BE: CW 15-1023, AIFSN 3
         * BK: CW 15-1023, AIFSN 7
         * VI: CW 7-15, AIFSN 2, TXOP 3008 usec
         * VO: CW 3-7, AIFSN 2, TXOP 1504 usec
    Country: EU Environment: Indoor/Outdoor
        Channels [1 - 13] @ 16 dBm
BSS 34:31:c4:b8:2e:85(on wlan0)
    TSF: 212081672689 usec (2d, 10:54:41)
    freq: 2437
    beacon interval: 100 TUs
    capability: ESS Privacy ShortPreamble ShortSlotTime RadioMeasure (0x1431)
    signal: -83.00 dBm
    last seen: 28400 ms ago
    Information elements from Probe Response frame:
    SSID: Nexus
    Supported rates: 1.0* 2.0* 5.5* 11.0* 6.0* 9.0 12.0* 18.0 
    DS Parameter set: channel 6
    TIM: DTIM Count 0 DTIM Period 1 Bitmap Control 0x0 Bitmap[0] 0x0 (+ 1 octet)
    Country: DE Environment: Indoor/Outdoor
        Channels [1 - 13] @ 20 dBm
    ERP: <no flags>
    Extended supported rates: 24.0* 36.0 48.0 54.0 
    BSS Load:
         * station count: 13
         * channel utilisation: 74/255
         * available admission capacity: 0 [*32us]
    HT capabilities:
        Capabilities: 0x1ad
            RX LDPC
            HT20
            SM Power Save disabled
            RX HT20 SGI
            TX STBC
            RX STBC 1-stream
            Max AMSDU length: 3839 bytes
            No DSSS/CCK HT40
        Maximum RX AMPDU length 65535 bytes (exponent: 0x003)
        Minimum RX AMPDU time spacing: 8 usec (0x06)
        HT TX/RX MCS rate indexes supported: 0-23
    HT operation:
         * primary channel: 6
         * secondary channel offset: no secondary
         * STA channel width: 20 MHz
         * RIFS: 0
         * HT protection: nonmember
         * non-GF present: 1
         * OBSS non-GF present: 0
         * dual beacon: 0
         * dual CTS protection: 0
         * STBC beacon: 0
         * L-SIG TXOP Prot: 0
         * PCO active: 0
         * PCO phase: 0
    Overlapping BSS scan params:
         * passive dwell: 20 TUs
         * active dwell: 10 TUs
         * channel width trigger scan interval: 300 s
         * scan passive total per channel: 200 TUs
         * scan active total per channel: 20 TUs
         * BSS width channel transition delay factor: 5
         * OBSS Scan Activity Threshold: 0.25 %
    Extended capabilities: HT Information Exchange Supported, Extended Channel Switching, TFS, WNM-Sleep Mode, TIM Broadcast, BSS Transition, 6
    WMM:     * Parameter version 1
         * BE: CW 15-1023, AIFSN 3
         * BK: CW 15-1023, AIFSN 7
         * VI: CW 7-15, AIFSN 2, TXOP 3008 usec
         * VO: CW 3-7, AIFSN 2, TXOP 1504 usec
    WPS:     * Version: 1.0
         * Wi-Fi Protected Setup State: 2 (Configured)
         * RF Bands: 0x3
         * Unknown TLV (0x1049, 6 bytes): 00 37 2a 00 01 20
    RSN:     * Version: 1
         * Group cipher: CCMP
         * Pairwise ciphers: CCMP
         * Authentication suites: PSK 00-0f-ac:8
         * Capabilities: 1-PTKSA-RC 1-GTKSA-RC MFP-capable (0x0080)
BSS 92:5c:14:db:21:48(on wlan0)
    TSF: 212098644532 usec (2d, 10:54:58)
    freq: 2462
    beacon interval: 100 TUs
    capability: ESS ShortSlotTime RadioMeasure (0x1401)
    signal: -71.00 dBm
    last seen: 11430 ms ago
    Information elements from Probe Response frame:
    SSID: Vodafone Hotspot
    Supported rates: 1.0* 2.0* 5.5* 11.0* 9.0 18.0 36.0 54.0 
    DS Parameter set: channel 11
    ERP: Barker_Preamble_Mode
    Extended supported rates: 6.0 12.0 24.0 48.0 
    Country: EU Environment: Indoor/Outdoor
        Channels [1 - 13] @ 20 dBm
    HT capabilities:
        Capabilities: 0x1ac
            HT20
            SM Power Save disabled
            RX HT20 SGI
            TX STBC
            RX STBC 1-stream
            Max AMSDU length: 3839 bytes
            No DSSS/CCK HT40
        Maximum RX AMPDU length 65535 bytes (exponent: 0x003)
        Minimum RX AMPDU time spacing: 4 usec (0x05)
        HT RX MCS rate indexes supported: 0-15
        HT TX MCS rate indexes are undefined
    HT operation:
         * primary channel: 11
         * secondary channel offset: no secondary
         * STA channel width: 20 MHz
         * RIFS: 0
         * HT protection: no
         * non-GF present: 1
         * OBSS non-GF present: 0
         * dual beacon: 0
         * dual CTS protection: 0
         * STBC beacon: 0
         * L-SIG TXOP Prot: 0
         * PCO active: 0
         * PCO phase: 0
    Extended capabilities: HT Information Exchange Supported, BSS Transition
    BSS Load:
         * station count: 1
         * channel utilisation: 111/255
         * available admission capacity: 31250 [*32us]
    WMM:     * Parameter version 1
         * BE: CW 15-1023, AIFSN 3
         * BK: CW 15-1023, AIFSN 7
         * VI: CW 7-15, AIFSN 2, TXOP 3008 usec
         * VO: CW 3-7, AIFSN 2, TXOP 1504 usec
    Country: EU Environment: Indoor/Outdoor
        Channels [1 - 13] @ 16 dBm
BSS 9c:80:df:31:03:a4(on wlan0)
    TSF: 212082583134 usec (2d, 10:54:42)
    freq: 2467
    beacon interval: 100 TUs
    capability: ESS Privacy ShortSlotTime (0x0411)
    signal: -87.00 dBm
    last seen: 27490 ms ago
    Information elements from Probe Response frame:
    SSID: o2-WLAN84
    Supported rates: 1.0* 2.0* 5.5* 11.0* 9.0 18.0 36.0 54.0 
    DS Parameter set: channel 12
    Extended supported rates: 6.0 12.0 24.0 48.0 
    Country: DE Environment: Indoor/Outdoor
        Channels [1 - 13] @ 20 dBm
    WPS:     * Version: 1.0
         * Wi-Fi Protected Setup State: 2 (Configured)
    TIM: DTIM Count 0 DTIM Period 1 Bitmap Control 0x0 Bitmap[0] 0x0
    ERP: Barker_Preamble_Mode
    HT capabilities:
        Capabilities: 0x106e
            HT20/HT40
            SM Power Save disabled
            RX HT20 SGI
            RX HT40 SGI
            No RX STBC
            Max AMSDU length: 3839 bytes
            DSSS/CCK HT40
        Maximum RX AMPDU length 65535 bytes (exponent: 0x003)
        Minimum RX AMPDU time spacing: 4 usec (0x05)
        HT RX MCS rate indexes supported: 0-15, 32
        HT TX MCS rate indexes are undefined
    HT operation:
         * primary channel: 12
         * secondary channel offset: no secondary
         * STA channel width: 20 MHz
         * RIFS: 0
         * HT protection: 20 MHz
         * non-GF present: 1
         * OBSS non-GF present: 0
         * dual beacon: 0
         * dual CTS protection: 0
         * STBC beacon: 0
         * L-SIG TXOP Prot: 0
         * PCO active: 0
         * PCO phase: 0
    Extended capabilities: HT Information Exchange Supported
    Overlapping BSS scan params:
         * passive dwell: 20 TUs
         * active dwell: 10 TUs
         * channel width trigger scan interval: 300 s
         * scan passive total per channel: 200 TUs
         * scan active total per channel: 20 TUs
         * BSS width channel transition delay factor: 5
         * OBSS Scan Activity Threshold: 0.25 %
    RSN:     * Version: 1
         * Group cipher: CCMP
         * Pairwise ciphers: CCMP
         * Authentication suites: PSK
         * Capabilities: PreAuth 1-PTKSA-RC 1-GTKSA-RC (0x0001)
    WMM:     * Parameter version 1
         * BE: CW 15-1023, AIFSN 3
         * BK: CW 15-1023, AIFSN 7
         * VI: CW 7-15, AIFSN 2, TXOP 3008 usec
         * VO: CW 3-7, AIFSN 2, TXOP 1504 usec
    BSS Load:
         * station count: 768
         * channel utilisation: 33/255
         * available admission capacity: 4730 [*32us]
BSS 36:2c:94:34:3b:95(on wlan0)
    TSF: 212096926483 usec (2d, 10:54:56)
    freq: 2412
    beacon interval: 100 TUs
    capability: ESS ShortSlotTime RadioMeasure (0x1401)
    signal: -84.00 dBm
    last seen: 13150 ms ago
    SSID: Vodafone Hotspot
    Supported rates: 1.0* 2.0* 5.5* 11.0* 9.0 18.0 36.0 54.0 
    DS Parameter set: channel 1
    ERP: Barker_Preamble_Mode
    Extended supported rates: 6.0 12.0 24.0 48.0 
    Country: EU Environment: Indoor/Outdoor
        Channels [1 - 13] @ 20 dBm
    HT capabilities:
        Capabilities: 0x1ac
            HT20
            SM Power Save disabled
            RX HT20 SGI
            TX STBC
            RX STBC 1-stream
            Max AMSDU length: 3839 bytes
            No DSSS/CCK HT40
        Maximum RX AMPDU length 65535 bytes (exponent: 0x003)
        Minimum RX AMPDU time spacing: 4 usec (0x05)
        HT RX MCS rate indexes supported: 0-15
        HT TX MCS rate indexes are undefined
    HT operation:
         * primary channel: 1
         * secondary channel offset: no secondary
         * STA channel width: 20 MHz
         * RIFS: 0
         * HT protection: no
         * non-GF present: 0
         * OBSS non-GF present: 0
         * dual beacon: 0
         * dual CTS protection: 0
         * STBC beacon: 0
         * L-SIG TXOP Prot: 0
         * PCO active: 0
         * PCO phase: 0
    Extended capabilities: HT Information Exchange Supported, BSS Transition
    BSS Load:
         * station count: 0
         * channel utilisation: 90/255
         * available admission capacity: 31250 [*32us]
    WMM:     * Parameter version 1
         * BE: CW 15-1023, AIFSN 3
         * BK: CW 15-1023, AIFSN 7
         * VI: CW 7-15, AIFSN 2, TXOP 3008 usec
         * VO: CW 3-7, AIFSN 2, TXOP 1504 usec
    Country: EU Environment: Indoor/Outdoor
        Channels [1 - 13] @ 16 dBm
BSS 38:43:7d:1c:95:e6(on wlan0)
    TSF: 212097695148 usec (2d, 10:54:57)
    freq: 2437
    beacon interval: 100 TUs
    capability: ESS Privacy ShortSlotTime RadioMeasure (0x1411)
    signal: -83.00 dBm
    last seen: 12380 ms ago
    Information elements from Probe Response frame:
    SSID: UPCB45EF15
    Supported rates: 1.0* 2.0* 5.5* 11.0* 9.0 18.0 36.0 54.0 
    DS Parameter set: channel 6
    Extended supported rates: 6.0 12.0 24.0 48.0 
    Country: EU Environment: Indoor/Outdoor
        Channels [1 - 13] @ 20 dBm
    TIM: DTIM Count 0 DTIM Period 1 Bitmap Control 0x0 Bitmap[0] 0x0
    WPA:     * Version: 1
         * Group cipher: TKIP
         * Pairwise ciphers: TKIP CCMP
         * Authentication suites: PSK
    RSN:     * Version: 1
         * Group cipher: TKIP
         * Pairwise ciphers: TKIP CCMP
         * Authentication suites: PSK
         * Capabilities: 1-PTKSA-RC 1-GTKSA-RC (0x0000)
    WPS:     * Version: 1.0
         * Wi-Fi Protected Setup State: 2 (Configured)
         * UUID: 30b60e80-1dd2-11b2-8601-8e4aa01a9d4a
         * RF Bands: 0x1
         * Unknown TLV (0x1049, 6 bytes): 00 37 2a 00 01 20
    ERP: Barker_Preamble_Mode
    HT capabilities:
        Capabilities: 0x1ac
            HT20
            SM Power Save disabled
            RX HT20 SGI
            TX STBC
            RX STBC 1-stream
            Max AMSDU length: 3839 bytes
            No DSSS/CCK HT40
        Maximum RX AMPDU length 65535 bytes (exponent: 0x003)
        Minimum RX AMPDU time spacing: 4 usec (0x05)
        HT RX MCS rate indexes supported: 0-15
        HT TX MCS rate indexes are undefined
    HT operation:
         * primary channel: 6
         * secondary channel offset: no secondary
         * STA channel width: 20 MHz
         * RIFS: 0
         * HT protection: no
         * non-GF present: 1
         * OBSS non-GF present: 0
         * dual beacon: 0
         * dual CTS protection: 0
         * STBC beacon: 0
         * L-SIG TXOP Prot: 0
         * PCO active: 0
         * PCO phase: 0
    Extended capabilities: HT Information Exchange Supported, BSS Transition
    WMM:     * Parameter version 1
         * BE: CW 15-1023, AIFSN 3
         * BK: CW 15-1023, AIFSN 7
         * VI: CW 7-15, AIFSN 2, TXOP 3008 usec
         * VO: CW 3-7, AIFSN 2, TXOP 1504 usec
    BSS Load:
         * station count: 1
         * channel utilisation: 86/255
         * available admission capacity: 31250 [*32us]
BSS 90:5c:44:db:21:33(on wlan0)
    TSF: 212107555845 usec (2d, 10:55:07)
    freq: 5180
    beacon interval: 100 TUs
    capability: ESS Privacy ShortPreamble SpectrumMgmt ShortSlotTime RadioMeasure (0x1531)
    signal: -88.00 dBm
    last seen: 2510 ms ago
    Information elements from Probe Response frame:
    SSID: UPC614F5E5
    Supported rates: 6.0* 9.0 12.0* 18.0 24.0* 36.0 48.0 54.0 
    DS Parameter set: channel 36
    Power constraint: 3 dB
    RSN:     * Version: 1
         * Group cipher: TKIP
         * Pairwise ciphers: CCMP
         * Authentication suites: PSK
         * Capabilities: 1-PTKSA-RC 1-GTKSA-RC (0x0000)
    HT capabilities:
        Capabilities: 0x6f
            RX LDPC
            HT20/HT40
            SM Power Save disabled
            RX HT20 SGI
            RX HT40 SGI
            No RX STBC
            Max AMSDU length: 3839 bytes
            No DSSS/CCK HT40
        Maximum RX AMPDU length 65535 bytes (exponent: 0x003)
        Minimum RX AMPDU time spacing: 4 usec (0x05)
        HT RX MCS rate indexes supported: 0-23, 32
        HT TX MCS rate indexes are undefined
    HT operation:
         * primary channel: 36
         * secondary channel offset: above
         * STA channel width: any
         * RIFS: 0
         * HT protection: no
         * non-GF present: 1
         * OBSS non-GF present: 0
         * dual beacon: 0
         * dual CTS protection: 0
         * STBC beacon: 0
         * L-SIG TXOP Prot: 0
         * PCO active: 0
         * PCO phase: 0
    Extended capabilities: 6
    VHT capabilities:
        VHT Capabilities (0x33827930):
            Max MPDU length: 3895
            Supported Channel Width: neither 160 nor 80+80
            RX LDPC
            short GI (80 MHz)
            SU Beamformer
            SU Beamformee
            RX antenna pattern consistency
            TX antenna pattern consistency
        VHT RX MCS set:
            1 streams: MCS 0-9
            2 streams: MCS 0-9
            3 streams: MCS 0-9
            4 streams: not supported
            5 streams: not supported
            6 streams: not supported
            7 streams: not supported
            8 streams: not supported
        VHT RX highest supported: 0 Mbps
        VHT TX MCS set:
            1 streams: MCS 0-9
            2 streams: MCS 0-9
            3 streams: MCS 0-9
            4 streams: not supported
            5 streams: not supported
            6 streams: not supported
            7 streams: not supported
            8 streams: not supported
        VHT TX highest supported: 0 Mbps
    VHT operation:
         * channel width: 1 (80 MHz)
         * center freq segment 1: 42
         * center freq segment 2: 0
         * VHT basic MCS set: 0xffc0
    BSS Load:
         * station count: 2
         * channel utilisation: 54/255
         * available admission capacity: 30000 [*32us]
    WPA:     * Version: 1
         * Group cipher: TKIP
         * Pairwise ciphers: TKIP
         * Authentication suites: PSK
    WMM:     * Parameter version 1
         * u-APSD
         * BE: CW 15-1023, AIFSN 3
         * BK: CW 15-1023, AIFSN 7
         * VI: CW 7-15, AIFSN 2, TXOP 3008 usec
         * VO: CW 3-7, AIFSN 2, TXOP 1504 usec
    WPS:     * Version: 1.0
         * Wi-Fi Protected Setup State: 2 (Configured)
         * Response Type: 3 (AP)
         * UUID: 314ea500-1dd2-11b2-8601-8e4aa01a9d4a
         * Manufacturer: Marvell
         * Model: WAP
         * Model Number: 123
         * Serial Number: 12345
         * Primary Device Type: 6-0050f204-1
         * Device name: 5G wireless AP
         * Config methods:
         * RF Bands: 0x2
         * Unknown TLV (0x1049, 6 bytes): 00 37 2a 00 01 20
BSS a8:d3:f7:96:10:6d(on wlan0)
    TSF: 212107799783 usec (2d, 10:55:07)
    freq: 5200
    beacon interval: 100 TUs
    capability: ESS Privacy SpectrumMgmt ShortSlotTime (0x0511)
    signal: -88.00 dBm
    last seen: 2260 ms ago
    Information elements from Probe Response frame:
    SSID: o2-WLAN34
    Supported rates: 6.0* 9.0 12.0* 18.0 24.0 36.0 48.0 54.0 
    DS Parameter set: channel 40
    Country: DE Environment: Indoor/Outdoor
        Channels [36 - 36] @ 23 dBm
        Channels [40 - 40] @ 23 dBm
        Channels [44 - 44] @ 23 dBm
        Channels [48 - 48] @ 23 dBm
    Power constraint: 0 dB
    HT capabilities:
        Capabilities: 0x86f
            RX LDPC
            HT20/HT40
            SM Power Save disabled
            RX HT20 SGI
            RX HT40 SGI
            No RX STBC
            Max AMSDU length: 7935 bytes
            No DSSS/CCK HT40
        Maximum RX AMPDU length 65535 bytes (exponent: 0x003)
        Minimum RX AMPDU time spacing: 4 usec (0x05)
        HT TX/RX MCS rate indexes supported: 0-31, 33-76
    HT operation:
         * primary channel: 40
         * secondary channel offset: below
         * STA channel width: any
         * RIFS: 0
         * HT protection: nonmember
         * non-GF present: 1
         * OBSS non-GF present: 1
         * dual beacon: 0
         * dual CTS protection: 0
         * STBC beacon: 0
         * L-SIG TXOP Prot: 0
         * PCO active: 0
         * PCO phase: 0
    WMM:     * Parameter version 1
         * u-APSD
         * BE: CW 15-1023, AIFSN 3
         * BK: CW 15-1023, AIFSN 7
         * VI: CW 7-15, AIFSN 2, TXOP 3008 usec
         * VO: CW 3-7, AIFSN 2, TXOP 1504 usec
    RSN:     * Version: 1
         * Group cipher: CCMP
         * Pairwise ciphers: CCMP
         * Authentication suites: PSK
         * Capabilities: 1-PTKSA-RC 1-GTKSA-RC (0x0000)
    Extended capabilities: HT Information Exchange Supported, SSID List, 6
    WPS:     * Version: 1.0
         * Wi-Fi Protected Setup State: 2 (Configured)
         * Response Type: 3 (AP)
         * UUID: 4e9bd57c-8ebe-46d8-aa04-cdd3994f7288
         * Manufacturer: Quantenna
         * Model: Topaz
         * Model Number: QV840.432
         * Serial Number: A8D3F796106D
         * Primary Device Type: 6-0050f204-1
         * Device name: Reference Design
         * Config methods:
         * Unknown TLV (0x1049, 6 bytes): 00 37 2a 00 01 20
    VHT capabilities:
        VHT Capabilities (0x3fcb7832):
            Max MPDU length: 11454
            Supported Channel Width: neither 160 nor 80+80
            RX LDPC
            short GI (80 MHz)
            SU Beamformer
            SU Beamformee
            MU Beamformer
            +HTC-VHT
            RX antenna pattern consistency
            TX antenna pattern consistency
        VHT RX MCS set:
            1 streams: MCS 0-9
            2 streams: MCS 0-9
            3 streams: MCS 0-9
            4 streams: MCS 0-9
            5 streams: not supported
            6 streams: not supported
            7 streams: not supported
            8 streams: not supported
        VHT RX highest supported: 0 Mbps
        VHT TX MCS set:
            1 streams: MCS 0-9
            2 streams: MCS 0-9
            3 streams: MCS 0-9
            4 streams: MCS 0-9
            5 streams: not supported
            6 streams: not supported
            7 streams: not supported
            8 streams: not supported
        VHT TX highest supported: 0 Mbps
    VHT operation:
         * channel width: 1 (80 MHz)
         * center freq segment 1: 42
         * center freq segment 2: 0
         * VHT basic MCS set: 0xfffc
BSS 90:5c:44:d1:34:20(on wlan0)
    TSF: 212108016406 usec (2d, 10:55:08)
    freq: 5220
    beacon interval: 100 TUs
    capability: ESS Privacy ShortPreamble SpectrumMgmt ShortSlotTime RadioMeasure (0x1531)
    signal: -46.00 dBm
    last seen: 2060 ms ago
    Information elements from Probe Response frame:
    SSID: UPC5144FAF
    Supported rates: 6.0* 9.0 12.0* 18.0 24.0* 36.0 48.0 54.0 
    DS Parameter set: channel 44
    Power constraint: 3 dB
    RSN:     * Version: 1
         * Group cipher: TKIP
         * Pairwise ciphers: CCMP
         * Authentication suites: PSK
         * Capabilities: 1-PTKSA-RC 1-GTKSA-RC (0x0000)
    HT capabilities:
        Capabilities: 0x6f
            RX LDPC
            HT20/HT40
            SM Power Save disabled
            RX HT20 SGI
            RX HT40 SGI
            No RX STBC
            Max AMSDU length: 3839 bytes
            No DSSS/CCK HT40
        Maximum RX AMPDU length 65535 bytes (exponent: 0x003)
        Minimum RX AMPDU time spacing: 4 usec (0x05)
        HT RX MCS rate indexes supported: 0-23, 32
        HT TX MCS rate indexes are undefined
    HT operation:
         * primary channel: 44
         * secondary channel offset: above
         * STA channel width: any
         * RIFS: 0
         * HT protection: no
         * non-GF present: 1
         * OBSS non-GF present: 0
         * dual beacon: 0
         * dual CTS protection: 0
         * STBC beacon: 0
         * L-SIG TXOP Prot: 0
         * PCO active: 0
         * PCO phase: 0
    Extended capabilities: 6
    VHT capabilities:
        VHT Capabilities (0x33827930):
            Max MPDU length: 3895
            Supported Channel Width: neither 160 nor 80+80
            RX LDPC
            short GI (80 MHz)
            SU Beamformer
            SU Beamformee
            RX antenna pattern consistency
            TX antenna pattern consistency
        VHT RX MCS set:
            1 streams: MCS 0-9
            2 streams: MCS 0-9
            3 streams: MCS 0-9
            4 streams: not supported
            5 streams: not supported
            6 streams: not supported
            7 streams: not supported
            8 streams: not supported
        VHT RX highest supported: 0 Mbps
        VHT TX MCS set:
            1 streams: MCS 0-9
            2 streams: MCS 0-9
            3 streams: MCS 0-9
            4 streams: not supported
            5 streams: not supported
            6 streams: not supported
            7 streams: not supported
            8 streams: not supported
        VHT TX highest supported: 0 Mbps
    VHT operation:
         * channel width: 1 (80 MHz)
         * center freq segment 1: 42
         * center freq segment 2: 0
         * VHT basic MCS set: 0xffc0
    BSS Load:
         * station count: 1
         * channel utilisation: 33/255
         * available admission capacity: 30000 [*32us]
    WPA:     * Version: 1
         * Group cipher: TKIP
         * Pairwise ciphers: TKIP
         * Authentication suites: PSK
    WMM:     * Parameter version 1
         * u-APSD
         * BE: CW 15-1023, AIFSN 3
         * BK: CW 15-1023, AIFSN 7
         * VI: CW 7-15, AIFSN 2, TXOP 3008 usec
         * VO: CW 3-7, AIFSN 2, TXOP 1504 usec
    WPS:     * Version: 1.0
         * Wi-Fi Protected Setup State: 2 (Configured)
         * Response Type: 3 (AP)
         * UUID: 30b60e80-1dd2-11b2-8601-8e4aa01a9d4a
         * Manufacturer: Marvell
         * Model: WAP
         * Model Number: 123
         * Serial Number: 12345
         * Primary Device Type: 6-0050f204-1
         * Device name: 5G wireless AP
         * Config methods:
         * RF Bands: 0x2
         * Unknown TLV (0x1049, 6 bytes): 00 37 2a 00 01 20
BSS ac:22:05:db:4d:22(on wlan0)
    TSF: 212108018921 usec (2d, 10:55:08)
    freq: 5220
    beacon interval: 100 TUs
    capability: ESS Privacy ShortPreamble SpectrumMgmt ShortSlotTime RadioMeasure (0x1531)
    signal: -68.00 dBm
    last seen: 2020 ms ago
    Information elements from Probe Response frame:
    SSID: Hoeheitsgebiet
    Supported rates: 6.0* 9.0 12.0* 18.0 24.0* 36.0 48.0 54.0 
    DS Parameter set: channel 44
    Power constraint: 3 dB
    RSN:     * Version: 1
         * Group cipher: TKIP
         * Pairwise ciphers: CCMP
         * Authentication suites: PSK
         * Capabilities: 1-PTKSA-RC 1-GTKSA-RC (0x0000)
    HT capabilities:
        Capabilities: 0x6f
            RX LDPC
            HT20/HT40
            SM Power Save disabled
            RX HT20 SGI
            RX HT40 SGI
            No RX STBC
            Max AMSDU length: 3839 bytes
            No DSSS/CCK HT40
        Maximum RX AMPDU length 65535 bytes (exponent: 0x003)
        Minimum RX AMPDU time spacing: 4 usec (0x05)
        HT RX MCS rate indexes supported: 0-23, 32
        HT TX MCS rate indexes are undefined
    HT operation:
         * primary channel: 44
         * secondary channel offset: above
         * STA channel width: any
         * RIFS: 0
         * HT protection: no
         * non-GF present: 1
         * OBSS non-GF present: 0
         * dual beacon: 0
         * dual CTS protection: 0
         * STBC beacon: 0
         * L-SIG TXOP Prot: 0
         * PCO active: 0
         * PCO phase: 0
    Extended capabilities: 6
    VHT capabilities:
        VHT Capabilities (0x33827930):
            Max MPDU length: 3895
            Supported Channel Width: neither 160 nor 80+80
            RX LDPC
            short GI (80 MHz)
            SU Beamformer
            SU Beamformee
            RX antenna pattern consistency
            TX antenna pattern consistency
        VHT RX MCS set:
            1 streams: MCS 0-9
            2 streams: MCS 0-9
            3 streams: MCS 0-9
            4 streams: not supported
            5 streams: not supported
            6 streams: not supported
            7 streams: not supported
            8 streams: not supported
        VHT RX highest supported: 0 Mbps
        VHT TX MCS set:
            1 streams: MCS 0-9
            2 streams: MCS 0-9
            3 streams: MCS 0-9
            4 streams: not supported
            5 streams: not supported
            6 streams: not supported
            7 streams: not supported
            8 streams: not supported
        VHT TX highest supported: 0 Mbps
    VHT operation:
         * channel width: 1 (80 MHz)
         * center freq segment 1: 42
         * center freq segment 2: 0
         * VHT basic MCS set: 0xffc0
    BSS Load:
         * station count: 4
         * channel utilisation: 43/255
         * available admission capacity: 30000 [*32us]
    WPA:     * Version: 1
         * Group cipher: TKIP
         * Pairwise ciphers: TKIP
         * Authentication suites: PSK
    WMM:     * Parameter version 1
         * u-APSD
         * BE: CW 15-1023, AIFSN 3
         * BK: CW 15-1023, AIFSN 7
         * VI: CW 7-15, AIFSN 2, TXOP 3008 usec
         * VO: CW 3-7, AIFSN 2, TXOP 1504 usec
    WPS:     * Version: 1.0
         * Wi-Fi Protected Setup State: 2 (Configured)
         * Response Type: 3 (AP)
         * UUID: 327fd200-1dd2-11b2-8601-8e4aa01a9d4a
         * Manufacturer: Marvell
         * Model: WAP
         * Model Number: 123
         * Serial Number: 12345
         * Primary Device Type: 6-0050f204-1
         * Device name: 5G wireless AP
         * Config methods:
         * RF Bands: 0x2
         * Unknown TLV (0x1049, 6 bytes): 00 37 2a 00 01 20
BSS 54:67:51:2c:3d:0a(on wlan0)
    TSF: 212108254184 usec (2d, 10:55:08)
    freq: 2462
    beacon interval: 100 TUs
    capability: ESS Privacy ShortSlotTime RadioMeasure (0x1411)
    signal: -80.00 dBm
    last seen: 1820 ms ago
    Information elements from Probe Response frame:
    SSID: UPC956E146
    Supported rates: 1.0* 2.0* 5.5* 11.0* 9.0 18.0 36.0 54.0 
    DS Parameter set: channel 11
    ERP: Barker_Preamble_Mode
    Extended supported rates: 6.0 12.0 24.0 48.0 
    Country: EU Environment: Indoor/Outdoor
        Channels [1 - 13] @ 20 dBm
    HT capabilities:
        Capabilities: 0x1ac
            HT20
            SM Power Save disabled
            RX HT20 SGI
            TX STBC
            RX STBC 1-stream
            Max AMSDU length: 3839 bytes
            No DSSS/CCK HT40
        Maximum RX AMPDU length 65535 bytes (exponent: 0x003)
        Minimum RX AMPDU time spacing: 4 usec (0x05)
        HT RX MCS rate indexes supported: 0-15
        HT TX MCS rate indexes are undefined
    HT operation:
         * primary channel: 11
         * secondary channel offset: no secondary
         * STA channel width: 20 MHz
         * RIFS: 0
         * HT protection: no
         * non-GF present: 0
         * OBSS non-GF present: 0
         * dual beacon: 0
         * dual CTS protection: 0
         * STBC beacon: 0
         * L-SIG TXOP Prot: 0
         * PCO active: 0
         * PCO phase: 0
    WPA:     * Version: 1
         * Group cipher: TKIP
         * Pairwise ciphers: TKIP CCMP
         * Authentication suites: PSK
    RSN:     * Version: 1
         * Group cipher: TKIP
         * Pairwise ciphers: TKIP CCMP
         * Authentication suites: PSK
         * Capabilities: 1-PTKSA-RC 1-GTKSA-RC (0x0000)
    Extended capabilities: HT Information Exchange Supported, BSS Transition
    BSS Load:
         * station count: 0
         * channel utilisation: 93/255
         * available admission capacity: 31250 [*32us]
    WMM:     * Parameter version 1
         * BE: CW 15-1023, AIFSN 3
         * BK: CW 15-1023, AIFSN 7
         * VI: CW 7-15, AIFSN 2, TXOP 3008 usec
         * VO: CW 3-7, AIFSN 2, TXOP 1504 usec
    Country: EU Environment: Indoor/Outdoor
        Channels [1 - 13] @ 16 dBm
    WPS:     * Version: 1.0
         * Wi-Fi Protected Setup State: 2 (Configured)
         * Response Type: 3 (AP)
         * UUID: 314ea500-1dd2-11b2-8601-8e4aa01a9d4a
         * Manufacturer: Ralink Technology, Corp.
         * Model: Ralink Wireless Access Point
         * Model Number: RT2860
         * Serial Number: 12345678
         * Primary Device Type: 6-0050f204-1
         * Device name: RalinkAPS
         * Config methods:
         * RF Bands: 0x1
         * Unknown TLV (0x1049, 6 bytes): 00 37 2a 00 01 20
BSS 74:31:70:75:f1:e2(on wlan0)
    TSF: 212098649788 usec (2d, 10:54:58)
    freq: 2462
    beacon interval: 100 TUs
    capability: ESS Privacy ShortSlotTime (0x0411)
    signal: -80.00 dBm
    last seen: 11420 ms ago
    Information elements from Probe Response frame:
    SSID: WLAN-75F122
    Supported rates: 1.0* 2.0* 5.5* 11.0* 18.0 24.0 36.0 54.0 
    DS Parameter set: channel 11
    ERP: <no flags>
    ERP D4.0: <no flags>
    RSN:     * Version: 1
         * Group cipher: CCMP
         * Pairwise ciphers: CCMP
         * Authentication suites: PSK
         * Capabilities: 1-PTKSA-RC 1-GTKSA-RC (0x0000)
    Extended supported rates: 6.0 9.0 12.0 48.0 
    HT capabilities:
        Capabilities: 0x186c
            HT20
            SM Power Save disabled
            RX HT20 SGI
            RX HT40 SGI
            No RX STBC
            Max AMSDU length: 7935 bytes
            DSSS/CCK HT40
        Maximum RX AMPDU length 65535 bytes (exponent: 0x003)
        Minimum RX AMPDU time spacing: 16 usec (0x07)
        HT RX MCS rate indexes supported: 0-15
        HT TX MCS rate indexes are undefined
    HT operation:
         * primary channel: 11
         * secondary channel offset: no secondary
         * STA channel width: 20 MHz
         * RIFS: 1
         * HT protection: no
         * non-GF present: 1
         * OBSS non-GF present: 0
         * dual beacon: 0
         * dual CTS protection: 0
         * STBC beacon: 0
         * L-SIG TXOP Prot: 0
         * PCO active: 0
         * PCO phase: 0
    Overlapping BSS scan params:
         * passive dwell: 20 TUs
         * active dwell: 10 TUs
         * channel width trigger scan interval: 300 s
         * scan passive total per channel: 200 TUs
         * scan active total per channel: 20 TUs
         * BSS width channel transition delay factor: 5
         * OBSS Scan Activity Threshold: 0.25 %
    Extended capabilities: HT Information Exchange Supported
    WMM:     * Parameter version 1
         * BE: CW 15-1023, AIFSN 3
         * BK: CW 15-1023, AIFSN 7
         * VI: CW 7-15, AIFSN 2, TXOP 3008 usec
         * VO: CW 3-7, AIFSN 2, TXOP 1504 usec
    WPS:     * Version: 1.0
         * Wi-Fi Protected Setup State: 2 (Configured)
         * Selected Registrar: 0x0
         * Response Type: 3 (AP)
         * UUID: 00000000-0000-0003-0000-74317075f1e2
         * Manufacturer: Corporation
         * Model: VGV8539JW
         * Model Number: 1.47.000
         * Serial Number: J144024542
         * Primary Device Type: 6-0050f204-1
         * Device name: Wireless Router(WFA)
         * Config methods: Label, PBC
         * RF Bands: 0x3
BSS 1c:b0:44:75:42:a8(on wlan0)
    TSF: 212108018214 usec (2d, 10:55:08)
    freq: 5220
    beacon interval: 100 TUs
    capability: ESS Privacy SpectrumMgmt ShortSlotTime (0x0511)
    signal: -89.00 dBm
    last seen: 2060 ms ago
    SSID: o2-WLAN38
    Supported rates: 6.0* 9.0 12.0* 18.0 24.0 36.0 48.0 54.0 
    DS Parameter set: channel 44
    BSS Load:
         * station count: 5
         * channel utilisation: 55/255
         * available admission capacity: 65535 [*32us]
    Country: DE Environment: Indoor/Outdoor
        Channels [36 - 36] @ 23 dBm
        Channels [40 - 40] @ 23 dBm
        Channels [44 - 44] @ 23 dBm
        Channels [48 - 48] @ 23 dBm
    Power constraint: 0 dB
    HT capabilities:
        Capabilities: 0x86f
            RX LDPC
            HT20/HT40
            SM Power Save disabled
            RX HT20 SGI
            RX HT40 SGI
            No RX STBC
            Max AMSDU length: 7935 bytes
            No DSSS/CCK HT40
        Maximum RX AMPDU length 65535 bytes (exponent: 0x003)
        Minimum RX AMPDU time spacing: 4 usec (0x05)
        HT TX/RX MCS rate indexes supported: 0-31, 33-76
    HT operation:
         * primary channel: 44
         * secondary channel offset: above
         * STA channel width: any
         * RIFS: 0
         * HT protection: nonmember
         * non-GF present: 1
         * OBSS non-GF present: 1
         * dual beacon: 0
         * dual CTS protection: 0
         * STBC beacon: 0
         * L-SIG TXOP Prot: 0
         * PCO active: 0
         * PCO phase: 0
    WMM:     * Parameter version 1
         * u-APSD
         * BE: CW 15-1023, AIFSN 3
         * BK: CW 15-1023, AIFSN 7
         * VI: CW 7-15, AIFSN 2, TXOP 3008 usec
         * VO: CW 3-7, AIFSN 2, TXOP 1504 usec
    RSN:     * Version: 1
         * Group cipher: CCMP
         * Pairwise ciphers: CCMP
         * Authentication suites: PSK
         * Capabilities: 1-PTKSA-RC 1-GTKSA-RC MFP-capable (0x0080)
         * 0 PMKIDs
         * Group mgmt cipher suite: AES-128-CMAC
    Extended capabilities: HT Information Exchange Supported, BSS Transition, SSID List, 6
    WPS:     * Version: 1.0
         * Wi-Fi Protected Setup State: 2 (Configured)
         * Response Type: 3 (AP)
         * UUID: b0493afc-202d-11b2-8a5b-1cb0447542a5
         * Manufacturer: Askey
         * Model: o2 HomeBox
         * Model Number: 6741
         * Serial Number: 1CB0447542A8
         * Primary Device Type: 6-0050f204-1
         * Device name: o2 HomeBox 6741
         * Config methods: Display
         * Unknown TLV (0x1049, 6 bytes): 00 37 2a 00 01 20
    VHT capabilities:
        VHT Capabilities (0x3fcb7832):
            Max MPDU length: 11454
            Supported Channel Width: neither 160 nor 80+80
            RX LDPC
            short GI (80 MHz)
            SU Beamformer
            SU Beamformee
            MU Beamformer
            +HTC-VHT
            RX antenna pattern consistency
            TX antenna pattern consistency
        VHT RX MCS set:
            1 streams: MCS 0-9
            2 streams: MCS 0-9
            3 streams: MCS 0-9
            4 streams: MCS 0-9
            5 streams: not supported
            6 streams: not supported
            7 streams: not supported
            8 streams: not supported
        VHT RX highest supported: 0 Mbps
        VHT TX MCS set:
            1 streams: MCS 0-9
            2 streams: MCS 0-9
            3 streams: MCS 0-9
            4 streams: MCS 0-9
            5 streams: not supported
            6 streams: not supported
            7 streams: not supported
            8 streams: not supported
        VHT TX highest supported: 0 Mbps
    VHT operation:
         * channel width: 1 (80 MHz)
         * center freq segment 1: 42
         * center freq segment 2: 0
         * VHT basic MCS set: 0xfffc