            CPU0       CPU1       
   0:         18          0   IO-APIC    2-edge      timer
   1:          0         73   IO-APIC    1-edge      i8042
   8:          1          0   IO-APIC    8-edge      rtc0
   9:          0          0   IO-APIC    9-fasteoi   acpi
  12:         18          0   IO-APIC   12-edge      i8042
  14:          0          0   IO-APIC   14-edge      ata_piix
  15:          0          0   IO-APIC   15-edge      ata_piix
  16:       3545          0   IO-APIC   16-fasteoi   vmwgfx, snd_ens1371
  17:      33795          0   IO-APIC   17-fasteoi   ehci_hcd:usb1, ioc0
  18:          0     368326   IO-APIC   18-fasteoi   uhci_hcd:usb2
  19:          0     126705   IO-APIC   19-fasteoi   ens33
  24:          0          0   PCI-MSI 344064-edge      PCIe PME, pciehp
  25:          0          0   PCI-MSI 346112-edge      PCIe PME, pciehp
  26:          0          0   PCI-MSI 348160-edge      PCIe PME, pciehp
  27:          0          0   PCI-MSI 350208-edge      PCIe PME, pciehp
  28:          0          0   PCI-MSI 352256-edge      PCIe PME, pciehp
  29:          0          0   PCI-MSI 354304-edge      PCIe PME, pciehp
  30:          0          0   PCI-MSI 356352-edge      PCIe PME, pciehp
  31:          0          0   PCI-MSI 358400-edge      PCIe PME, pciehp
  32:          0          0   PCI-MSI 360448-edge      PCIe PME, pciehp
  33:          0          0   PCI-MSI 362496-edge      PCIe PME, pciehp
  34:          0          0   PCI-MSI 364544-edge      PCIe PME, pciehp
  35:          0          0   PCI-MSI 366592-edge      PCIe PME, pciehp
  36:          0          0   PCI-MSI 368640-edge      PCIe PME, pciehp
  37:          0          0   PCI-MSI 370688-edge      PCIe PME, pciehp
  38:          0          0   PCI-MSI 372736-edge      PCIe PME, pciehp
  39:          0          0   PCI-MSI 374784-edge      PCIe PME, pciehp
  40:          0          0   PCI-MSI 376832-edge      PCIe PME, pciehp
  41:          0          0   PCI-MSI 378880-edge      PCIe PME, pciehp
  42:          0          0   PCI-MSI 380928-edge      PCIe PME, pciehp
  43:          0          0   PCI-MSI 382976-edge      PCIe PME, pciehp
  44:          0          0   PCI-MSI 385024-edge      PCIe PME, pciehp
  45:          0          0   PCI-MSI 387072-edge      PCIe PME, pciehp
  46:          0          0   PCI-MSI 389120-edge      PCIe PME, pciehp
  47:          0          0   PCI-MSI 391168-edge      PCIe PME, pciehp
  48:          0          0   PCI-MSI 393216-edge      PCIe PME, pciehp
  49:          0          0   PCI-MSI 395264-edge      PCIe PME, pciehp
  50:          0          0   PCI-MSI 397312-edge      PCIe PME, pciehp
  51:          0          0   PCI-MSI 399360-edge      PCIe PME, pciehp
  52:          0          0   PCI-MSI 401408-edge      PCIe PME, pciehp
  53:          0          0   PCI-MSI 403456-edge      PCIe PME, pciehp
  54:          0          0   PCI-MSI 405504-edge      PCIe PME, pciehp
  55:          0          0   PCI-MSI 407552-edge      PCIe PME, pciehp
  56:          0       7937   PCI-MSI 1130496-edge      ahci[0000:02:05.0]
  57:          0       2061   PCI-MSI 129024-edge      vmw_vmci
  58:          0          0   PCI-MSI 129025-edge      vmw_vmci
 NMI:          0          0   Non-maskable interrupts
 LOC:     366351     997227   Local timer interrupts
 SPU:          0          0   Spurious interrupts
 PMI:          0          0   Performance monitoring interrupts
 IWI:          0          3   IRQ work interrupts
 RTR:          0          0   APIC ICR read retries
 RES:       2763       2933   Rescheduling interrupts
 CAL:     175136     130374   Function call interrupts
 TLB:       3155       3965   TLB shootdowns
 TRM:          0          0   Thermal event interrupts
 THR:          0          0   Threshold APIC interrupts
 DFR:          0          0   Deferred Error APIC interrupts
 MCE:          0          0   Machine check exceptions
 MCP:         49         50   Machine check polls
 ERR:          0
 MIS:          0
 PIN:          0          0   Posted-interrupt notification event
 NPI:          0          0   Nested posted-interrupt event
 PIW:          0          0   Posted-interrupt wakeup event
